/*****************************************************************************
 *	Copyright(c) 2007,  RealTEK Technology Inc. All Right Reserved.
 *  
 *	Realtek RTL8192S PCI-E 802.11B/G/N 300M Wireless NIC Release Note. 
 *	
 *	Description:	
 *					N.VVVV.DDDD.YYYY
 *					N		-	NDIS number
 *					VVVV	-	Version	1001	-->
 *					DDDD	-	Data	10/19	-->
 *					YYYY	-	Year	2007	-->	
 * 
 *****************************************************************************/


############################################################################
	Version:		
	5.1010.0930.2008
	
	Reason:			
	1. Formal Release
----------------------------------------------------------------------------
############################################################################
	Version:		
	5.1020.1114.2007		
	
	Reason:			
	1. Fixs for interoperability performance test
----------------------------------------------------------------------------
############################################################################
	Version:		
	5.1030.1202.2007		
	
	Reason:			
	1. Fixs for performance fine tune in noisy environment
----------------------------------------------------------------------------
############################################################################
	Version:		
	5.1040.1216.2007		
	
	Reason:			
	1. Fixs for short and long distance throughput
							
----------------------------------------------------------------------------
############################################################################
	Version:		
	5.1050.1219.2007		
	
	Reason:			
	1. Throughput enhancement on Vista platform
	2. Fix QoS Id settings
	3. Improve throughput on 20MHz bandwidth
	4. Improve throughput with Netgear 854T
	5. Improve throughput with Cisco 1250 11N AP
							
----------------------------------------------------------------------------
############################################################################
	Version:		
	5.1065.0109.2009
	
	Reason:			
	1. Improve throughput stability by modify tx power setting
	2. Improve throughput in long distance
	3. Modification for DTM logo test
	4. Add smart roaming mechanism
	5. Lower power consumption
	
	Version:		
	5.1066.0115.2009
	
	Reason:
	1. Enable HW Radio on/off function

	Version:		
	5.1069.0123.2009
	
	Reason:
	1. Modification for DTM test
	2. Support Global Domain and WW-13 channel plan	

----------------------------------------------------------------------------	
############################################################################
	Version:		
	5.1070.0225.2009
	
	Reason:
	1. Improve LPS mechime.
	2. Improve throughput with broadcom/linksys AP.
	
	Version:
	5.1072.0304/2009
	
	Reason:
	1. Fine tune Ad-hoc throughput low issue
	2. Enhance Ad-hoc connection issue
	3. Enahcne the response time when user is accessing Internet Website.
	
	Version:
	5.1073.0304.2009
	
	Reason:
	1. Improve stability when s3/s4.
	
	Version:
	5.1074.0307.2009

	Reason:
	1. Support LED function
	
	Version:
	5.1075.0313.2009
	
	Reason:
	1. Improve stability for endurance test.
	2. Support options for link ANY operation. 
	3. Support Mutual Authentication

----------------------------------------------------------------------------
	Version:
	5.1076.0317.2009
	
	Reason:
	1. Modification for DTM only
	
	Version:
	1076.1.0320.2009
	1. Report correct connection status after s3/s4
	2. Clear connection state so that there will be no yellow band
	   after reboot.
	   
	   
	Version:
	1076.2.0324.2009
	1. Fix boot up issue on one specific platform
----------------------------------------------------------------------------
	Version:
	1077.0.0325.2009
	
	Reason:
	1. Midification for LED behavior
	
	
	Version:
	1077.1.0330.2009
	
	Reason:
	1. Modification for stability of s3/s4 long run test
	
----------------------------------------------------------------------------
	Version:
	1078.0.0401.2009
	
	Reason:
	1. Midification for RSSI
	2. fine tune cisco 1252AP throughput

	Version:
	1078.1.0402.2009
	
	Reason:
	1. Modify INF String
	
----------------------------------------------------------------------------
	Version:
	1079.0.0409.2009
	
	Reason:
	1. Modification for warm reboot long run test.
	2. Modification for yellow mark issue after s3/s4 on specific platform
	3. Associate 11N AP with G mode if encryption algorithm is set to TKIP
	   in order to follow WFA requirement.
	   
	Version:
	1079.1.0409.2009
	
	Reason:
	1. Modification for S3 long run test.

----------------------------------------------------------------------------
############################################################################
	Version:
	1080.0.0410.2009
	
	Reason:
	1. Modification for multiple language and LED strategy.
	
	Version:
	1080.1.0413.2009
	
	Reason:
	1. Improve IOT for Marvel AP.
	2. Add SDID/SVID for more customers.
	3. Improve link stablity when connect with different setting AP.
	
	Version:
	1080.2.0416.2009
	
	Reason:
	1. Improve IOT for Atheros AP.
	
	Version:
	1080.3.0416.2009
	
	Reason:
	1. Modify signal strength and signal quality policy for one customer.

----------------------------------------------------------------------------
	Version:
	1081.0.0421.2009
	
	Reason:
	1. Support B/G mode only for some countries.	
	2. Report disconnection if roaming fail for more than three times.
	
	Version:
	1081.1.0423.2009
	
	Reason:
	1. Modify for customer's power down requirement.
	
----------------------------------------------------------------------------
	Version:
	1082.0.0427.2009
	
	Reason:
	1. Improve throughput stability for long run test.
	2. Enable Tx power tracking scheme.
	
----------------------------------------------------------------------------
	Version:
	1083.0.0508.2009
	
	Reason:
	1. Do not enter power save mode if NIC is configured in "High Performance"
	2. Improve throughput with DIR655 and Netgear854T
	
----------------------------------------------------------------------------
	Version:
	1084.0.0522.2009
	
	Reason:
	1. Do not enter power save mode if Global Power Save Setting is configured 
	   in "High Performance"
	2. Add LED for customer
	3. WEP mode auto-connect after radio ON/OFF under Vista
	
----------------------------------------------------------------------------
  Version:
	1085.0.0611.2009
	
	Reason:
	1. Improve throughput with one specific GBT AP .
	2. Disable dynamic mechanism of 1x1 interoperability issue.
	3. Pass Low Temperature test.
	4. Get IPv6 IP successfully on one special condition
	5. Improve long run test stability.
	6. Add XP ADHOC WEP RF switch auto link.
	
		
	Version:
	1085.1.0612.2009
	
	Reason:
	1. Remove throughput improvement with GBT AP
	2. Remove IPv6 getting issue on one specific environment
	3. Remove XP ADHOC RF swith auto link
	
	Version:
	1085.2.0616.2009
	
	Reason:
	1. Get IPv6 successfully on one specific environment
	
	Version:
	1085.3.0618.2009
	
	Reason:
	1. It takes longer time at first resume on one specific platform
	
	Version:
	1085.4.0626.2009
	
	Reason:
	1. Modify mapping between data rate and link speed.
	
	Version:
	1085.4.0703.2009
	
	Reason:
	1. Support B/G only sku
	2. Support showing of Tx or Rx link speed based on customer request
	3. Fix adhoc can't be create on some situation

	Version:
	1085.5.0706.2009
	
	Reason:
	1. Fix a issue for customized platform
	
	Version:
	1085.6.0710.2009
	
	Reason:
	1. Pass Long run test on one specific platform
	
	Version:
	1085.7.0723.2009
	
	Reason:
	1. Support fix rate showing for one specific customer
	2. Support enable/disable link ANY function according to customer request.
	3. Fix not being able to ping success to peer specific ad-hoc STA under 
	   some special conditions.
	   
	Version:
	1085.7.0724.2009
	
	Reason:
	1. For pass WLK1.4   
	
	Version:
	1085.8.0727.2009
	
	Reason:
	1. Improve stability for a platform of one customer.
	
	Version:
	1085.9.0731.2009
	
	Reason:
	1. Support Customized TKIP in N mode and N mode ad-hoc. 	  
	2. Speed up connection time after resume from S3 in AES mode.
	3. Support new Calpella platform
	4. Enhance long run test stability on some specific platforms.
	
	Version:
	1085.10.0826.2009
	
	Reason:
	1. Add customize power policy.		

	Version:
	1085.11.0828.2009
	
	Reason:
	1. Protect thread sequence.

	Version:
	1085.11.0904.2009
	
	Reason:
	1. Fix power consumption issue of 1085.11.0828
	2. Modification for DTM test.

	Version:
	1085.12.0914.2009
	
	Reason:
	1. Fix specific UI link speed.	
	
	Version:
	1085.13.0921.2009
	
	Reason:
	1. Fix DC/AC switch and HW RF On Off issue.
	2. Save swrf status.

	Version:
	1085.14.0923.2009
	
	Reason:
	1. Fix abnormal disconnect with some APs.

	Version:
	1085.15.0925.2009
	
	Reason:
	1. Add customize LED feature.
	
	Version: 
	1085.16.0930.2009
	
	Reason
	1. ADD customize LED
	2. Fix copy and compare test fail issue.
	3. Fix interoperability with some AP.
	
	Version: 
	1085.17.1015.2009
	
	Reason
	1. ADD customize LED.
	2. Add BG only SKU.
	3. Fix suspend resume ASPM setting.
	
	Version: 
	1085.18.1023.2009
	
	Reason
	1. Add customized feature.
			
	Version: 
	1085.19.1027.2009
	
	Reason
	1. ADD customize LED.
	2. Fix vista rating issue.

	Version: 
	1085.20.1103.2009
	
	Reason
	1. Add Customize pci bridge setting.
		
	Version:
	1085.21.1123.2009
	
	Reason:
	1. Add Intel Promiscuous functionality.
	
	Version:
	1085.22.1214.2009
	
	Reason:
	1. Fix WPA TKIP with groupkey WEP connect and get IP issue.
	
----------------------------------------------------------------------------
	Version:
	1086.0.0120.2010
	
	Reason:
	1. Add power policy for a special customer.
	2. Add LED for customer
	3. Add IOT action for Realtek AP.


	Version:
	1086.1.0129.2010
	
	Reason:
	1. Fine tune throughput for a specific AP.
	
----------------------------------------------------------------------------	
	Version:
	1087.0.0210.2010
	
	Reason:
	1. Support WLK 1.5.
	2. Improve RF switch process.
	3. Support dynamic scan period to reduce scan time.
	4. Support dynamic security mode switch for customer.
	
----------------------------------------------------------------------------
	Version:
	1088.0.0313.2010
	
	Reason:
	1. Improve 1x1 one pair downlink.
	2. Fix customize RSSI.
	
	Version:
	1088.2.0319.2010
	
	Reason:
	1. Fix IOT issue with ipTime
	2. Speed up time for reporting disconnection after RF OFF

	Version:
	1088.3.0322.2010
	
	Reason:
	1. Cutomize behavior for link ANY	
	2. Improve 2x2 long distance TP 
		
----------------------------------------------------------------------------
	Version: 
	1089.0.0330.2010		
	1. Enable ASPM L1 in AMD platform by customer's request 
	2. Modify RF initialize behavior while enable and resume from S3/S4

	Version: 
	1089.1.0330.2010		
	1. add customize ID.
	
	Version: 
	1089.2.0401.2010		
	1. Regconize AMD Platform Releated setting by customized request.
	
----------------------------------------------------------------------------
	Version: 
	1090.0.0422.2010		
	1. Customized LED behavior
	2. Improve Ad-hoc mode stability
	3. Modifiation for BT-Coexistence
	
	Version: 
	1090.1.0427.2010		
	1. Fix BSOD issue to be compatible with McAfee 2010.
	
	Version: 
	1090.2.0504.2010		
	1. Fix BSOD issue due to illegal TKIP packet length.
	2. Disable debug component.
	
	Version: 
	1090.3.0517.2010		
	1. Modify TSB power consumption.
	2. Modify TKIP packet receive handler.

----------------------------------------------------------------------------
	Version: 
	1091.0.0520.2010		
	1. Modify power detection scheme for customer.
	
	Version: 
	1091.1.0521.2010		
	1. Modify ASPM setting for customer.
	
	Version: 
	1091.2.0521.2010		
	1. Correct ASPM setting for customer.
	2. Correct LED behavior for customer.
	
	Version: 
	1091.3.0607.2010		
	1. Modify ASPM setting for customer.

----------------------------------------------------------------------------
	Version: 
	1092.0.0628.2010		
	1. Improve init mechanism for customer.
	
	1092.1.0802.2010 (Vista/XP)			
	1. Modify to prevent multi device PCI configuration race condition.
	2. Modify for multi core thread race condition.

----------------------------------------------------------------------------
	Version: 
	1093.0.1108.2010		
	1. Update FW to fix power down nodule bug.
		
	1093.1.1207.2010
	1. Improve interoperability with Meru IOT
	
	1093.2.1215.2010
	1. Modify WW13 channel plan according to customer's requirement.
	2. Customerize rate display. 
	
	1093.3.0104.2011
	1. Wep only support G rate.
	2. Fix BOSD reported from customer.
	
	1093.4.0117.2011
	1. Do not filter WLCCP packet.
	
	1093.5.0128.2011
	1. Check status for allocate.

----------------------------------------------------------------------------	
	1094.0.0304.2011
	1. Fix interoperbility with marvell ap.
	
	1094.1.0420.2011
	1. Add customer LED behavior.
	
	1094.2.0616.2011
	1. use null frame for power save with some ap 

	1094.3.0817.2011
	1. Improve roaming IOT.


	1094.4.0907.2011
	1. Correct LED behavior during booting time.
