;; Realtek RTL8192SE PCI-E Wireless LAN Network Interface Cards.
;;
;; Copyright 1996-2007, Realtek Semiconductor Corporation
;;

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %Realtek%                                 ;;
CatalogFile.NT = net8192se.cat				   ;; for WHQL certified
DriverVer = 01/17/2012,1094.5.0117.2012

[Manufacturer]
%Realtek% = Realtek,NTx86
%Lenovo% = Lenovo,NTx86
		               

;;****************************************************************************
;; IDs for X86
;;****************************************************************************

[Realtek.NTx86]

%RTL8191seva.DeviceDesc%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8171
%RTL8191seva.DeviceDesc.HP%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8171&SUBSYS_1467103c
%RTL8191seva.DeviceDesc.HP%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8171&SUBSYS_817110ec
%RTL8191sevb.DeviceDesc%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172
%RTL8191sevb.DeviceDesc.PEGATRON%	= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_00941B0A
%RTL8191sevb.DeviceDesc.QMI%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_718510EC
%RTL8191sevb.DeviceDesc.QMI_EM308%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_03081A32
%RTL8191sevb.DeviceDesc.GBT%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_E93F1458
%RTL8192ge.DeviceDesc%			= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8173
%RTL8192se.DeviceDesc%			= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8174

%RTL8191seva.DeviceDesc.ASUS_G%		= AsusG.ndi,	PCI\VEN_10EC&DEV_8171&SUBSYS_1A071A3B
%RTL8191sevb.DeviceDesc.ASUS_G%		= AsusG.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_1A041A3B
%RTL8191seva.DeviceDesc.ASUS_N%		= AsusN.ndi,	PCI\VEN_10EC&DEV_8171&SUBSYS_11071A3B
%RTL8191sevb.DeviceDesc.ASUS_N%		= AsusN.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_11041A3B

%RTL8191seva.DeviceDesc.MSI_G%		= MsiG.ndi, PCI\VEN_10EC&DEV_8171&SUBSYS_897A1462
%RTL8191sevb.DeviceDesc.MSI_G%		= MsiG.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_897A1462
%RTL8191seva.DeviceDesc.MSI_N%		= MsiN.ndi, PCI\VEN_10EC&DEV_8171&SUBSYS_68971462
%RTL8191sevb.DeviceDesc.MSI_N%		= MsiN.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_68971462

;for lenovo
[Lenovo.NTx86]
%Lenovo.DeviceDesc%			= RTL8192se.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC

;;****************************************************************************
;; IDs for X64
;;****************************************************************************

[Realtek.NTamd64]

%RTL8191seva.DeviceDesc%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8171
%RTL8191seva.DeviceDesc.HP%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8171&SUBSYS_1467103c
%RTL8191seva.DeviceDesc.HP%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8171&SUBSYS_817110ec
%RTL8191sevb.DeviceDesc%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172
%RTL8191sevb.DeviceDesc.PEGATRON%	= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_00941B0A
%RTL8191sevb.DeviceDesc.QMI%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_718510EC
%RTL8191sevb.DeviceDesc.QMI_EM308%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_03081A32
%RTL8191sevb.DeviceDesc.GBT%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_E93F1458
%RTL8192ge.DeviceDesc%			= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8173
%RTL8192se.DeviceDesc%			= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8174

%RTL8191seva.DeviceDesc.ASUS_G%		= AsusG.ndi,	PCI\VEN_10EC&DEV_8171&SUBSYS_1A071A3B
%RTL8191sevb.DeviceDesc.ASUS_G%		= AsusG.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_1A041A3B
%RTL8191seva.DeviceDesc.ASUS_N%		= AsusN.ndi,	PCI\VEN_10EC&DEV_8171&SUBSYS_11071A3B
%RTL8191sevb.DeviceDesc.ASUS_N%		= AsusN.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_11041A3B

%RTL8191seva.DeviceDesc.MSI_G%		= MsiG.ndi, PCI\VEN_10EC&DEV_8171&SUBSYS_897A1462
%RTL8191sevb.DeviceDesc.MSI_G%		= MsiG.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_897A1462
%RTL8191seva.DeviceDesc.MSI_N%		= MsiN.ndi, PCI\VEN_10EC&DEV_8171&SUBSYS_68971462
%RTL8191sevb.DeviceDesc.MSI_N%		= MsiN.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_68971462

;for lenovo
[Lenovo.NTamd64]
%Lenovo.DeviceDesc%			= RTL8192se.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC

;;****************************************************************************
;; IDs for W2K
;;****************************************************************************

[Realtek]

%RTL8191seva.DeviceDesc%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8171
%RTL8191sevb.DeviceDesc%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172
%RTL8191sevb.DeviceDesc.PEGATRON%	= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_00941B0A
%RTL8191sevb.DeviceDesc.QMI%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_718510EC
%RTL8191sevb.DeviceDesc.QMI_EM308%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_03081A32
%RTL8191sevb.DeviceDesc.GBT%		= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8172&SUBSYS_E93F1458
%RTL8192ge.DeviceDesc%			= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8173
%RTL8192se.DeviceDesc%			= RTL8192se.ndi, 	PCI\VEN_10EC&DEV_8174

%RTL8191seva.DeviceDesc.ASUS_G%		= AsusG.ndi,	PCI\VEN_10EC&DEV_8171&SUBSYS_1A071A3B
%RTL8191sevb.DeviceDesc.ASUS_G%		= AsusG.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_1A041A3B
%RTL8191seva.DeviceDesc.ASUS_N%		= AsusN.ndi,	PCI\VEN_10EC&DEV_8171&SUBSYS_11071A3B
%RTL8191sevb.DeviceDesc.ASUS_N%		= AsusN.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_11041A3B

%RTL8191seva.DeviceDesc.MSI_G%		= MsiG.ndi, PCI\VEN_10EC&DEV_8171&SUBSYS_897A1462
%RTL8191sevb.DeviceDesc.MSI_G%		= MsiG.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_897A1462
%RTL8191seva.DeviceDesc.MSI_N%		= MsiN.ndi, PCI\VEN_10EC&DEV_8171&SUBSYS_68971462
%RTL8191sevb.DeviceDesc.MSI_N%		= MsiN.ndi, PCI\VEN_10EC&DEV_8172&SUBSYS_68971462

;for lenovo
[Lenovo]
%Lenovo.DeviceDesc%			= RTL8192se.ndi,	PCI\VEN_10EC&DEV_8172&SUBSYS_E02010EC

;;****************************************************************************
;; Windows 2000/XP
;;****************************************************************************
[RTL8192se.ndi.NT]
AddReg          = RTL8192se.common.reg, RTL8192se.reg, 11nWirelessMode.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8192se.CopyFiles

[RTL8192se.ndi.NT.Services]
AddService = RTL8192se, 2, RTL8192se.Service, RTL8192se.EventLog

[RTL8192se.CopyFiles]
rtl8192se.sys,,,2

[RTL8192se.CopyFiles98]
rtl8192se.sys,,,2

[AsusN.ndi.NT]
AddReg          = RTL8192se.common.reg, RTL8192se.reg, 11nAdhoc.reg, 11nWirelessMode.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8192se.CopyFiles

[AsusN.ndi.NT.Services]
AddService = RTL8192se, 2, RTL8192se.Service, RTL8192se.EventLog

[AsusG.ndi.NT]
AddReg          = RTL8192se.common.reg, RTL8192se.reg, 11gWirelessMode.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8192se.CopyFiles

[AsusG.ndi.NT.Services]
AddService = RTL8192se, 2, RTL8192se.Service, RTL8192se.EventLog

[MsiN.ndi.NT]
AddReg          = RTL8192se.common.reg, RTL8192se.reg, 11nWirelessMode.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8192se.CopyFiles

[MsiN.ndi.NT.Services]
AddService = RTL8192se, 2, RTL8192se.Service, RTL8192se.EventLog

[MsiG.ndi.NT]
AddReg          = RTL8192se.common.reg, RTL8192se.reg, 11gWirelessMode.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = RTL8192se.CopyFiles

[MsiG.ndi.NT.Services]
AddService = RTL8192se, 2, RTL8192se.Service, RTL8192se.EventLog

;;----------------------------------------------------------------------------
;; RTL8192se Parameters
;;----------------------------------------------------------------------------

;;****************************************************************************
;; RTL8192se common parameters
;;****************************************************************************
[11nAdhoc.reg]
HKR,Ndi\params\11nAdhoc,        ParamDesc,  0, %11NADHOC_ENABLE_STR%
HKR,Ndi\params\11nAdhoc,        type,       0, "enum"
HKR,Ndi\params\11nAdhoc,        default,    0, "0"
HKR,Ndi\params\11nAdhoc\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\11nAdhoc\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,11nAdhoc,0,"0"
HKR,,11nAdhoc,0,"0"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

[RTL8192se.common.reg]
HKR,defaults,		   AH_BcnIntv, 	0, "1000"
HKR,Ndi\params\AH_BcnIntv, default, 	0, "100"
HKR,Ndi\params\AH_BcnIntv, ParamDesc, 	0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, type, 	0, "int"
HKR,Ndi\params\AH_BcnIntv, min, 	0, "20"
HKR,Ndi\params\AH_BcnIntv, max, 	0, "1000"
HKR,Ndi\params\AH_BcnIntv, step, 	0, "1"

HKR,Ndi\params\Dot11dEnable,        ParamDesc,  0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable,        type,       0, "enum"
HKR,Ndi\params\Dot11dEnable,        default,    0, "0"
HKR,Ndi\params\Dot11dEnable\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"

;Roaming Sensitivity Level
HKR,Ndi\Params\RegROAMSensitiveLevel, ParamDesc, 0, %ROAMING_SENSITIVITY_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel, Type,      0, "enum"
HKR,Ndi\Params\RegROAMSensitiveLevel, Default,   0, "3"
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "0",  0, %DISABLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "1",  0, %HIGH_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "2",  0, %MIDDLE_STR%
HKR,Ndi\Params\RegROAMSensitiveLevel\enum, "3",  0, %LOW_STR%

HKR,Ndi\params\PreambleMode,        ParamDesc,  0, %PREAMBLE_MODE_STR%
HKR,Ndi\params\PreambleMode,        type,       0, "enum"
HKR,Ndi\params\PreambleMode,        default,    0, "2"
HKR,Ndi\params\PreambleMode\enum,   "1",        0, %LONG_PREAMBLE_STR%
HKR,Ndi\params\PreambleMode\enum,   "2",        0, %LONG_SHORT_PREAMBLE_STR%
HKR,defaults,PreambleMode,0,"2"
HKR,,PreambleMode,0,"2"

HKR,Ndi\params\TxPowerLevel,        ParamDesc,  0, %TX_POWER_LEVEL_STR%
HKR,Ndi\params\TxPowerLevel,        type,       0, "enum"
HKR,Ndi\params\TxPowerLevel,        default,    0, "0"
HKR,Ndi\params\TxPowerLevel\enum,   "0",        0, %AUTO_STR%
HKR,Ndi\params\TxPowerLevel\enum,   "1",        0, %HIGH_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum,   "2",        0, %MIDDLE_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum,   "3",        0, %LOW_TX_POWER_STR%
HKR,Ndi\params\TxPowerLevel\enum,   "4",        0, %VERY_LOW_TX_POWER_STR%
HKR,defaults,TxPowerLevel,0,"0"
HKR,,TxPowerLevel,0,"0"

HKR,,Channel,0,"10"

;Inactive Power Save
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"2"
HKR,,bLeisurePs,0,"2"

;; ASPM
HKR,defaults,PciASPM,0,"2"
HKR,,PciASPM,0,"2"

;HKR,defaults,DevicePciASPMSetting,0,"3"
HKR,,DevicePciASPMSetting,0,"3"

;HKR,defaults,HostPciASPMSetting,0,"3"
HKR,,HostPciASPMSetting,0,"2"

;; RF Off
;HKR,defaults,HwSwRfOffD3,0,"2"
HKR,,HwSwRfOffD3,0,"2"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;; HW Radio ON/OFF Switch Polling.
;HKR,defaults,GPIORFSW,0,"1"
HKR,,GPIORFSW,0,"1"

;Keep Alive Mechanism
HKR,,KeepAliveLevel,0,"1"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"0"
HKR,,bFwCtrlLPS,0,"0"

; TKIP in N mode for Asus
HKR,,TKIPinNmode,0,"0"

; Show max rx rate for Asus
HKR,,ShowRate,0,"0"

;Clo Control Flag
HKR,defaults,CloEnable,0,"0"
HKR,,CloEnable,0,"0"

;Security Mode Flag
HKR,defaults,WepMode,0,"1"
HKR,,WepMode,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,,WiFiConfg,,"0"

;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"500"
HKR,,GPIOBack,0,"250"

;; For Host/Device ASPM setting.
HKR,,ASPMDelayFlag,0,"1"
HKR,,ASPMDelay,0,"20"

;;****************************************************************************
;; NT 5.0 parameters
;;****************************************************************************
[RTL8192se.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "RTL8192se"

[RTL8192se.Service]
DisplayName     = %RTL8192se.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\rtl8192se.sys
LoadOrderGroup  = NDIS

[RTL8192se.EventLog]
Addreg = RTL8192se.AddEventLog.reg

[RTL8192se.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
RTL8192se.CopyFiles           = 12
RTL8192se.CopyFiles98         = 11
DefaultDestDir                = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
rtl8192se.sys  = 1


;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
Realtek     				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"

TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Disable"
ENABLE_STR 				= "Enable"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"


FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR			= "Leisure Power Save"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"			


;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0009] ; English
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Channel"
NETWORK_TYPE_STR 			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
CHANNEL_PLAN_STR			= "Channel Plan"
WL_MODE_STR				= "Wireless Mode"
PREAMBLE_MODE_STR			= "Preamble Mode"
FRAGTHRESH_STR				= "Fragmentation Threshold"
RTSTHRESH_STR				= "RTS Threshold"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Disable"
ENABLE_STR 				= "Enable"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Auto select"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR			= "Leisure Power Save"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "25 %"			

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0404] ; Chinese (Traditional)
Realtek					= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "服務組合識別碼"
CHANNEL_STR				= "通訊頻道"
NETWORK_TYPE_STR 			= "無線網路操作模式"
LED_CONTROL_STR				= "驅動程式控制 LED 閃爍模式" 
POWER_SAVE_STR				= "省電模式"
WIFI_IBSS_STR				= "對等式網路只使用 802.11b 標準"
RATE_ADAPTIVE_STR			= "適應性傳輸率調變自動化模式"
QOS_STR					= "流量管控"
WMM_APSD				= "WiFi 多媒體自動化省電參數 (WMM APSD)"
CCX_RM_STR				= "CCX 無線網路環境監控"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 非連線頻道最大量測時間 (0: 無限大)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "支援 PSP XLink 連線模式"
CHANNEL_PLAN_STR			= "頻道規劃"
WL_MODE_STR				= "無線網路標準"
PREAMBLE_MODE_STR			= "前序訊號模式"
FRAGTHRESH_STR				= "區段臨界值"
RTSTHRESH_STR				= "RTS 臨界值"
DOT11_ENABLE_STR			= "802.11d 無線頻道區域規範"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "啟用"
CAM_STR 				= "無"
MAX_PSP_STR 				= "最大"
FAST_PSP_STR 				= "最小"
AD_HOC_STR 				= "對等式網路"
INFRASTRUCTURE_STR 			= "主從式網路"
AUTO_SELECT_STR 			= "自動選擇"
DOMAIN_FROM_EEPROM_STR 			= "硬體決定"
AUTO_STR 				= "自動選擇"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"

IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "漫遊重試限制（秒）"
LEISURE_POWER_SAVE_STR			= "空閒電力節省"
AH_BCNINTV_STR 				= "信標間隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "25 %"			

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"


;;====================================================================================================================
[Strings.0011] ; Japanese
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "チャンネル"
NETWORK_TYPE_STR 			= "ネットワークの種類"
LED_CONTROL_STR				= "LEDコントロール" 
POWER_SAVE_STR				= "省電力モード"
WIFI_IBSS_STR				= "IBSS既定11bモード"
RATE_ADAPTIVE_STR			= "適応レート"
QOS_STR					= "QoS "
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCXラジオ測定"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX最大オフライン測定（0: 無制限）"
FORCE_PRIORITY_STR			= "強制実行優先順位"
HW_PARA_STR				= "HwParaFileからのInit "
THREE_WIRE_MODE_STR			= "三線式プログラミングモード"
BOARD_TYPE_STR				= "基板の種類"
PROTECTION_MODE_STR			= "保護モード"
TPC_STR					= "送信電力制御"
TPC_POLARITY_STR			= "TPC極性選択"
HIGH_POWER_STR				= "高出力機構"
INIT_GAIN_STR				= "初期ゲイン状態"
CW_MAX_MIN_STR				= "コンテンションウィンドウ"
PSP_XLINK_STR				= "PSP XLinkモード"
CHANNEL_PLAN_STR			= "チャンネルプラン"
WL_MODE_STR				= "ワイヤレスモード"
PREAMBLE_MODE_STR			= "プレアンブルモード"
FRAGTHRESH_STR				= "フラグメンテーションしきい値"
RTSTHRESH_STR				= "RTSしきい値"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "無効"
ENABLE_STR 				= "有効"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "臨時"
INFRASTRUCTURE_STR 			= "インフラストラクチャ"
AUTO_SELECT_STR 			= "自動選択"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "自動"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "スペイン"
FRANCE_STR 				= "フランス"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "イスラエル"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "ローミング再試行制限 (秒)"
LEISURE_POWER_SAVE_STR			= "レジャーパワーセーブ"
AH_BCNINTV_STR 				= "ビーコン間隔"


ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "25 %"			


;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"


;;====================================================================================================================
[Strings.0007] ; German
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Netzwerktyp"
LED_CONTROL_STR				= "LED-Anzeige" 
POWER_SAVE_STR				= "Energiesparmodus"
WIFI_IBSS_STR				= "IBSS Default 11b Modus"
RATE_ADAPTIVE_STR			= "Ratenadaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Funkmessung"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max. Offline Messung (0: unbeschrankt)"
FORCE_PRIORITY_STR			= "Erzwungene Prioritat"
HW_PARA_STR				= "Init. von HwParaFile"
THREE_WIRE_MODE_STR			= "Dreileiter-Programmiermodus"
BOARD_TYPE_STR				= "Kartentyp"
PROTECTION_MODE_STR			= "Schutzmodus"
TPC_STR					= "Ubertragungsleistungsstuerung"
TPC_POLARITY_STR			= "TPC Polaritatsauswahl"
HIGH_POWER_STR				= "Hochleistungsmechanismus"
INIT_GAIN_STR				= "Anfangl. Verstarkungszustand"
CW_MAX_MIN_STR				= "Konkurrenz-Fenster"
PSP_XLINK_STR				= "PSP XLink Modus"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Wireless-Modus"
PREAMBLE_MODE_STR			= "Praambelmodus"
FRAGTHRESH_STR				= "Fragmentierungsschwelle"
RTSTHRESH_STR				= "RTS-Schwelle:"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Deaktivieren"
ENABLE_STR 				= "Aktivieren"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autom. Auswahl"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankreich"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Roaming-Wiederholungslimit (Sek.)"
LEISURE_POWER_SAVE_STR			= "Leerlauf-Energiesparen"
AH_BCNINTV_STR 				= "Bakenintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"


;;====================================================================================================================
[Strings.000c] ; French
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Type de reseau"
LED_CONTROL_STR				= "Commande DEL" 
POWER_SAVE_STR				= "Mode economie d'energie"
WIFI_IBSS_STR				= "Mode 11b par defaut IBSS"
RATE_ADAPTIVE_STR			= "Debit adaptable"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Mesure radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Mesure hors ligne max. (0: illimitee)"
FORCE_PRIORITY_STR			= "Priorite forcee"

HW_PARA_STR				= "Init de HwParaFile"
THREE_WIRE_MODE_STR			= "Mode de programmation trois fils"
BOARD_TYPE_STR				= "Type de carte"
PROTECTION_MODE_STR			= "Mode de protection"
TPC_STR					= "Transmission du reglage"
TPC_POLARITY_STR			= "Choix de la polarite TPC"
HIGH_POWER_STR				= "Mecanisme grande puissance"
INIT_GAIN_STR				= "Etat du gain initial"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "Mode XLink PSP"
CHANNEL_PLAN_STR			= "Plan de canal"
WL_MODE_STR				= "Mode sans fil"
PREAMBLE_MODE_STR			= "Mode preambule"
FRAGTHRESH_STR				= "Seuil de fragmentation"
RTSTHRESH_STR				= "Seuil RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Desactiver"
ENABLE_STR 				= "Activer"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastructure"
AUTO_SELECT_STR 			= "Selection automatique"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espagne"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Limite essais roam (sec)"
LEISURE_POWER_SAVE_STR			= "Economie d'energie loisirs"
AH_BCNINTV_STR 				= "Intervalle balise "

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0010] ; Italian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canale"
NETWORK_TYPE_STR 			= "Tipo di rete"
LED_CONTROL_STR				= "Controllo LED" 
POWER_SAVE_STR				= "Modalita risparmio energetico"
WIFI_IBSS_STR				= "Modalita IBBS predefinita 11b"
RATE_ADAPTIVE_STR			= "Si adatta alla velocita"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Misurazione radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Misurazione CCD max non in linea (0: illimitata)"
FORCE_PRIORITY_STR			= "Priorita forzata"
HW_PARA_STR				= "Init da HwParaFile"
THREE_WIRE_MODE_STR			= "Tre modalita di programmazione cablata"
BOARD_TYPE_STR				= "Tipo di piastra"

PROTECTION_MODE_STR			= "Modalita protezione"
TPC_STR					= "Trasmissione risparmio energetico"
TPC_POLARITY_STR			= "Selezione della polarita TPC"
HIGH_POWER_STR				= "Meccanismo ad alto potenziale"
INIT_GAIN_STR				= "Stato di guadagno iniziale"
CW_MAX_MIN_STR				= "Finestra di competizione"
PSP_XLINK_STR				= "Modalita PSP XLink"
CHANNEL_PLAN_STR			= "Piano canale"
WL_MODE_STR				= "Modalita wireless"
PREAMBLE_MODE_STR			= "Modalita preambolo"
FRAGTHRESH_STR				= "Soglia di frammentazione"
RTSTHRESH_STR				= "Soglia RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Disabilita"
ENABLE_STR 				= "Abilita"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruttura"
AUTO_SELECT_STR 			= "Selezione automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spagna"
FRANCE_STR 				= "Francia"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israele"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Limite tentativi roam (sec)"
LEISURE_POWER_SAVE_STR			= "Risparmio energetico tempo libero"
AH_BCNINTV_STR 				= "Beacon Interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"


;;====================================================================================================================
[Strings.000a] ; Spanish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Tipo de red"
LED_CONTROL_STR				= "Control de LED" 
POWER_SAVE_STR				= "Modo de ahorro de energia"
WIFI_IBSS_STR				= "Modo 11b predeterminado IBSS"
RATE_ADAPTIVE_STR			= "Velocidad adaptable"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Medicion de radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medicion sin conexion maxima CCX (0: sin limite)"
FORCE_PRIORITY_STR			= "Prioridad forzada"
HW_PARA_STR				= "Inicio desde HwParaFile"
THREE_WIRE_MODE_STR			= "Modo de programacion de tres cables"
BOARD_TYPE_STR				= "Tipo de tablero"
PROTECTION_MODE_STR			= "Modo de proteccion"
TPC_STR					= "Transmitir control de potencia"
TPC_POLARITY_STR			= "Seleccionar polaridad TPC"
HIGH_POWER_STR				= "Mecanismo de alta potencia"
INIT_GAIN_STR				= "Estado de ganancia inicial"
CW_MAX_MIN_STR				= "Ventana de discusiones"
PSP_XLINK_STR				= "Modo XLink PSP"
CHANNEL_PLAN_STR			= "Plan de canal"
WL_MODE_STR				= "Modo inalambrico"
PREAMBLE_MODE_STR			= "Modo de preambulo"
FRAGTHRESH_STR				= "Umbral de fragmentacion"
RTSTHRESH_STR				= "Umbral RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Deshabilitar"
ENABLE_STR 				= "Habilitar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "PSP_rapido"
AD_HOC_STR 				= "Especial"
INFRASTRUCTURE_STR 			= "Infraestructura"
AUTO_SELECT_STR 			= "Seleccion automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMINIO_DE_EEPROM"
AUTO_STR 				= "Automatico"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espana"
FRANCE_STR 				= "Francia"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Limite de reintentos en transito (seg)"
LEISURE_POWER_SAVE_STR			= "Ahorro de energia por inactividad"
AH_BCNINTV_STR 				= "Intervalo de baliza"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0c04] ; Chinese (Traditional) (Hong Kong)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR				= "服務組合識別碼"
CHANNEL_STR				= "通訊頻道"
NETWORK_TYPE_STR			= "無線網路操作模式"
LED_CONTROL_STR				= "驅動程式控制 LED 閃爍模式" 
POWER_SAVE_STR				= "省電模式"
WIFI_IBSS_STR				= "對等式網路只使用 802.11b 標準"
RATE_ADAPTIVE_STR			= "適應性傳輸率調變自動化模式"
QOS_STR					= "流量管控"
WMM_APSD				= "WiFi 多媒體自動化省電參數 (WMM APSD)"
CCX_RM_STR				= "CCX 無線網路環境監控"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 非連線頻道最大量測時間 (0: 無限大)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "支援 PSP XLink 連線模式"
CHANNEL_PLAN_STR			= "頻道規劃"
WL_MODE_STR				= "無線網路標準"
PREAMBLE_MODE_STR			= "前序訊號模式"
FRAGTHRESH_STR				= "區段臨界值"
RTSTHRESH_STR				= "RTS 臨界值"
DOT11_ENABLE_STR			= "802.11d 無線頻道區域規範"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "啟用"
CAM_STR 				= "無"
MAX_PSP_STR 				= "最大"
FAST_PSP_STR 				= "最小"
AD_HOC_STR 				= "對等式網路"
INFRASTRUCTURE_STR 			= "主從式網路"
AUTO_SELECT_STR 			= "自動選擇"
DOMAIN_FROM_EEPROM_STR 			= "硬體決定"
AUTO_STR 				= "自動選擇"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spain"
FRANCE_STR 				= "France"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "漫遊重試上限（秒）"
LEISURE_POWER_SAVE_STR			= "閑置中電源管理"
AH_BCNINTV_STR 				= "信標間隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0804] ; Chinese (Simplified)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "频道"
NETWORK_TYPE_STR 			= "网络类型"
LED_CONTROL_STR				= "LED 控制" 
POWER_SAVE_STR				= "省电模式"
WIFI_IBSS_STR				= "IBSS 默认 11b 模式"
RATE_ADAPTIVE_STR			= "速率适应"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX 无线电测量"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 最大脱机测量（0：无限制）"
FORCE_PRIORITY_STR			= "强制优先级"
HW_PARA_STR				= "从硬件参数文件初始化"
THREE_WIRE_MODE_STR			= "三线编程模式"
BOARD_TYPE_STR				= "板子类型"
PROTECTION_MODE_STR			= "保护模式"
TPC_STR					= "发射功率控制"
TPC_POLARITY_STR			= "TPC 极性选择"
HIGH_POWER_STR				= "高功率机制"
INIT_GAIN_STR				= "初始增益状态"
CW_MAX_MIN_STR				= "争用窗口"
PSP_XLINK_STR				= "PSP XLink 模式"
CHANNEL_PLAN_STR			= "频道计划"
WL_MODE_STR				= "无线模式"
PREAMBLE_MODE_STR			= "前导码模式"
FRAGTHRESH_STR				= "碎片阈值"
RTSTHRESH_STR				= "RTS 阈值"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "禁用"
ENABLE_STR 				= "启用"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "对等网络"
INFRASTRUCTURE_STR 			= "基础架构"
AUTO_SELECT_STR 			= "自动选择"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "自动"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "西班牙"
FRANCE_STR 				= "法国"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "以色列"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "漫游重试限制(秒)"
LEISURE_POWER_SAVE_STR			= "空闲省电"
AH_BCNINTV_STR 				= "信标间隔"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"


;;====================================================================================================================
[Strings.0012] ; Korean
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR				= "SSID"
CHANNEL_STR				= "채널"
NETWORK_TYPE_STR			= "네트워크 종류"
LED_CONTROL_STR				= "LED 제어" 
POWER_SAVE_STR				= "절전 모드"
WIFI_IBSS_STR				= "IBSS 기본 11b 모드"

RATE_ADAPTIVE_STR			= "속도 적응"
QOS_STR					= " QoS "
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX 무선 측정"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX 최대 오프라인 측정(0: 제한 없음)"
FORCE_PRIORITY_STR			= "강제 우선 순위"
HW_PARA_STR				= "HwParaFile에서 초기화"
THREE_WIRE_MODE_STR			= "3선 식 프로그래밍 모드"
BOARD_TYPE_STR				= "보드 종류"
PROTECTION_MODE_STR			= "보호 모드"

TPC_STR					= "송신 출력 제어"
TPC_POLARITY_STR			= "TPC 극성 선택"
HIGH_POWER_STR				= "고출력 메커니즘"
INIT_GAIN_STR				= "초기 게인 상태"
CW_MAX_MIN_STR				= "경합 창"
PSP_XLINK_STR				= "PSP XLink 모드"

CHANNEL_PLAN_STR			= "채널 계획"
WL_MODE_STR				= "무선 모드"
PREAMBLE_MODE_STR			= "프리앰블 모드"
FRAGTHRESH_STR 				= "조각화 임계값"
RTSTHRESH_STR				= "RTS 임계값"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "사용 안 함"
ENABLE_STR 				= "사용"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "애드혹"
INFRASTRUCTURE_STR 			= "인프라"
AUTO_SELECT_STR 			= "자동 선택"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "자동"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "스페인"
FRANCE_STR 				= "프랑스"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "이스라엘"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "로밍 재시도 제한시간(초)"
LEISURE_POWER_SAVE_STR			= "대기 절전"
AH_BCNINTV_STR 				= "비컨 간격"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"


;;====================================================================================================================
[Strings.0816] ; Portuguese (Portugal)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR 			= "Tipo de rede"
LED_CONTROL_STR				= "Controlo dos LEDs" 
POWER_SAVE_STR				= "Modo de poupanca de energia"
WIFI_IBSS_STR				= "Modo IBSS 11b predefinido"
RATE_ADAPTIVE_STR			= "Velocidade adaptativa"
QOS_STR					= "QoS"
WMM_APSD				= "APSD WMM"
CCX_RM_STR				= "Medida de radio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medida off-line maxima CCX (0: ilimitada)"
FORCE_PRIORITY_STR			= "Prioridade forcada"
HW_PARA_STR				= "Iniciar a partir de ficheiro de parametros do hardware"
THREE_WIRE_MODE_STR			= "Modo de programacao com tres fios"
BOARD_TYPE_STR				= "Tipo de placa"
PROTECTION_MODE_STR			= "Modo de proteccao"
TPC_STR					= "Controlo da potencia de transmissao"
TPC_POLARITY_STR			= "Seleccao da polaridade TPC"
HIGH_POWER_STR				= "Mecanismo de alta potencia"
INIT_GAIN_STR				= "Estado de ganho inicial"
CW_MAX_MIN_STR				= "Janela de contencao"
PSP_XLINK_STR				= "Modo PSP XLink"
CHANNEL_PLAN_STR			= "Plano de canais"
WL_MODE_STR				= "Modo sem fios"
PREAMBLE_MODE_STR			= "Modo de preambulo"
FRAGTHRESH_STR				= "Limiar de fragmentacao"
RTSTHRESH_STR				= "Limiar RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Desactivar"
ENABLE_STR 				= "Activar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infraestrutura"
AUTO_SELECT_STR 			= "Seleccao automatica"
DOMAIN_FROM_EEPROM_STR 			= "DOMINIO_DE_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanha"
FRANCE_STR 				= "Franca"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Limite para tentativas de itinerancia (seg.)"
LEISURE_POWER_SAVE_STR			= "Poupanca de energia em diversao"
AH_BCNINTV_STR 				= "Intervalo de sinalizacao"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0013] ; Dutch
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanaal"
NETWORK_TYPE_STR 			= "Netwerktype"
LED_CONTROL_STR				= "LED-besturing" 
POWER_SAVE_STR				= "Spaarstandmodus"
WIFI_IBSS_STR				= "IBSS standaard 11b-modus"
RATE_ADAPTIVE_STR			= "Aanpasbare snelheid"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX-radiometing"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX max. verschuivingsmeting (0: onbeperkt)"
FORCE_PRIORITY_STR			= "Geforceerde prioriteit"
HW_PARA_STR				= "Init van HwParaFile"
THREE_WIRE_MODE_STR			= "Driedraads programmeermodus"
BOARD_TYPE_STR				= "Bordtype"
PROTECTION_MODE_STR			= "Beveiligingsmodus"
TPC_STR					= "Zendvermogenbeheer"
TPC_POLARITY_STR			= "Selectie TPC-polariteit"

HIGH_POWER_STR				= "Mechanisme met hoog vermogen"
INIT_GAIN_STR				= "Eerste versterkingsstatus"
CW_MAX_MIN_STR				= "Conflictvenster"
PSP_XLINK_STR				= "PSP XLink-modus"
CHANNEL_PLAN_STR			= "Kanaalplan"
WL_MODE_STR				= "Draadloze modus"
PREAMBLE_MODE_STR			= "Preambulemodus"
FRAGTHRESH_STR				= "Fragmentatiedrempel"
RTSTHRESH_STR				= "RTS-drempel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Uitschakelen"
ENABLE_STR 				= "Inschakelen"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad hoc"
INFRASTRUCTURE_STR 			= "Infrastructuur"
AUTO_SELECT_STR 			= "Auto selectie"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanje"
FRANCE_STR 				= "Frankrijk"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Limiet van roamingspogingen(sec)"
LEISURE_POWER_SAVE_STR			= "Energiebesparing"
AH_BCNINTV_STR 				= "Bakeninterval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0014] ; Norwegian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Nettverkstype"
LED_CONTROL_STR				= "LED-kontroll" 
POWER_SAVE_STR				= "Stromsparingsmodus"
WIFI_IBSS_STR				= "IBSS standard 11b-modus"
RATE_ADAPTIVE_STR			= "Hastighet adaptiv"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radiomaling"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX maks offline-maling (0: ubegrenset)"
FORCE_PRIORITY_STR			= "Tvunget prioritet"
HW_PARA_STR				= "Init fra HwParaFile"
THREE_WIRE_MODE_STR			= "Tre tradet programmeringsmodus"
BOARD_TYPE_STR				= "Korttype"
PROTECTION_MODE_STR			= "Beskyttelsesmodus"
TPC_STR					= "Stromsendingskontroll"
TPC_POLARITY_STR			= "Velg TPC-polaritet"
HIGH_POWER_STR				= "Hoystyrke-mekanisme"
INIT_GAIN_STR				= "Opprinnelig okningstilstand"
CW_MAX_MIN_STR				= "Konflikt-vindu"
PSP_XLINK_STR				= "PSP XLink-modus"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Tradlos modus"
PREAMBLE_MODE_STR			= "Innledende modus"
FRAGTHRESH_STR				= "Fragmenteringsgrense"
RTSTHRESH_STR				= "RTS-grense"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Deaktiver"
ENABLE_STR 				= "Aktiver"
CAM_STR 				= "KAM"
MAX_PSP_STR 				= "MAKS_PSP"
FAST_PSP_STR 				= "Rask_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autovelg"
DOMAIN_FROM_EEPROM_STR 			= "DOMENE_FRA_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spania"
FRANCE_STR 				= "Frankrike"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Repeteringsgrense (i sek.) for roaming"
LEISURE_POWER_SAVE_STR			= "Stromsparing ved uvirksomhet"
AH_BCNINTV_STR 				= "Blinkintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.001d] ; Swedish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."


SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Natverkstyp"
LED_CONTROL_STR				= "LED-kontroll" 
POWER_SAVE_STR				= "Energisparlage"
WIFI_IBSS_STR				= "IBSS standard 11b Mode"
RATE_ADAPTIVE_STR			= "Anpassningsbar hastighet"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX radiomatning"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Offline matning (0: obegransat)"
FORCE_PRIORITY_STR			= "Tvingad prioritet"
HW_PARA_STR				= "Init fran HwParaFile"
THREE_WIRE_MODE_STR			= "Tretrads programmeringslage"
BOARD_TYPE_STR				= "Korttyp"
PROTECTION_MODE_STR			= "Skyddslage"
TPC_STR					= "Transmit Power Control"
TPC_POLARITY_STR			= "Valj TPC-polaritet"
HIGH_POWER_STR				= "Hogkraftsmekanism"
INIT_GAIN_STR				= "Ursprungligt forstarkningslage"
CW_MAX_MIN_STR				= "Konkurrensfonster"
PSP_XLINK_STR				= "PSP XLink-lage"
CHANNEL_PLAN_STR			= "Kanalplan"
WL_MODE_STR				= "Tradlost lage"
PREAMBLE_MODE_STR			= "Inledningslage"
FRAGTHRESH_STR				= "Fragmenteringstroskel"
RTSTHRESH_STR				= "RTS-troskel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Inaktivera"
ENABLE_STR 				= "Aktivera"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Autoval"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankrike"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Grans for nytt roamingforsok (sek)"
LEISURE_POWER_SAVE_STR			= "Leisure energibesparning"
AH_BCNINTV_STR 				= "Fyrintervall"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0006] ; Danish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Netvarkstype"
LED_CONTROL_STR				= "LED-kontrol" 
POWER_SAVE_STR				= "Stromstyrings-tilstand"
WIFI_IBSS_STR				= "IBSS standard 11b-tilstand"
RATE_ADAPTIVE_STR			= "Hastighed tilpasset"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX radiomaling"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX maks. offline-maling (0: ubegranset)"
FORCE_PRIORITY_STR			= "Forceret prioritet"
HW_PARA_STR				= "Init. fra HwParaFile"
THREE_WIRE_MODE_STR			= "Tre ledninger programmering-tilstand"
BOARD_TYPE_STR				= "Korttype"
PROTECTION_MODE_STR			= "Beskyttelse-tilstand"
TPC_STR					= "Overfor strom-kontrol"
TPC_POLARITY_STR			= "Valg TPC polaritet"
HIGH_POWER_STR				= "Hojeffekt-mekanisme"
INIT_GAIN_STR				= "Initiel forstarkning-tilstand"
CW_MAX_MIN_STR				= "Konflikt-vindue"
PSP_XLINK_STR				= "PSP XLink-tilstand"
CHANNEL_PLAN_STR			= "Kanal-plan"
WL_MODE_STR				= "Tradlos-tilstand"
PREAMBLE_MODE_STR			= "Start-tilstand"
FRAGTHRESH_STR				= "Fragmenteringstarskel"
RTSTHRESH_STR				= "RTS-tarskel"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Deaktiver"
ENABLE_STR 				= "Aktiver"
CAM_STR 				= "KAM"
MAX_PSP_STR 				= "MAKS._PSP"
FAST_PSP_STR 				= "Hurtig_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktur"
AUTO_SELECT_STR 			= "Auto-valg"
DOMAIN_FROM_EEPROM_STR 			= "DOMANE_FRA_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanien"
FRANCE_STR 				= "Frankrig"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Begransning for gentagne roam forsog (sek)"
LEISURE_POWER_SAVE_STR			= "Fritid - stromstyring"
AH_BCNINTV_STR 				= "Lys interval"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.000b] ; Finnsih
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."


SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanava"
NETWORK_TYPE_STR 			= "Verkkotyyppi"
LED_CONTROL_STR				= "LED-hallinta" 
POWER_SAVE_STR				= "Virransaastotila"
WIFI_IBSS_STR				= "IBSS-oletus 11b-tila"
RATE_ADAPTIVE_STR			= "Nopeuteen mukautuva"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX-radiomittaus"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX-maksimi-offline-mittaus (0: rajoittamaton)"
FORCE_PRIORITY_STR			= "Pakotettu prioriteetti"
HW_PARA_STR				= "Alustus HwParaFilesta"
THREE_WIRE_MODE_STR			= "Kolmen langan ohjelmointitila"
BOARD_TYPE_STR				= "Levytyyppi"
PROTECTION_MODE_STR			= "Suojaustila"
TPC_STR					= "Virranhallinnan siirto"
TPC_POLARITY_STR			= "TPC-polariteetin valinta"
HIGH_POWER_STR				= "Korkeatehomekanismi"
INIT_GAIN_STR				= "Ensimmainen vahvistustila"
CW_MAX_MIN_STR				= "Vaiteikkuna"
PSP_XLINK_STR				= "PSP XLink -tila"
CHANNEL_PLAN_STR			= "Kanavasuunnitelma"
WL_MODE_STR				= "Langaton tila"
PREAMBLE_MODE_STR			= "Synkronointitila"
FRAGTHRESH_STR				= "Sirpaleisuuden kynnys"
RTSTHRESH_STR				= "RTS-kynnys"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Pois paalta"
ENABLE_STR 				= "Paalle"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktuuri"
AUTO_SELECT_STR 			= "Automaattinen valinta"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Autom."
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanja"
FRANCE_STR 				= "Ranska"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Roamingin uudelleen yrittamisen rajoitus (sek.)"
LEISURE_POWER_SAVE_STR			= "Joutenolon virransaasto"
AH_BCNINTV_STR 				= "Paikkatietopakettien intervalli"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0019] ; Russian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Канал"
NETWORK_TYPE_STR 			= "Тип сети"
LED_CONTROL_STR				= "Индикатор" 
POWER_SAVE_STR				= "Режим энергосбережения"
WIFI_IBSS_STR				= "Режим IBSS Default 11b"
RATE_ADAPTIVE_STR			= "Адаптивная скорость"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: неограниченно)"
FORCE_PRIORITY_STR			= "Принудительный приоритет"
HW_PARA_STR				= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Режим Three Wire Programming Mode"
BOARD_TYPE_STR				= "Тип карты"
PROTECTION_MODE_STR			= "Защищенный режим"
TPC_STR					= "Управление мощностью передачи"
TPC_POLARITY_STR			= "Выбор полярности TPC"
HIGH_POWER_STR				= "Повышение мощности"
INIT_GAIN_STR				= "Первоначальное состояние усиления"
CW_MAX_MIN_STR				= "Окно соединения"
PSP_XLINK_STR				= "Режим PSP XLink"
CHANNEL_PLAN_STR			= "План каналов"
WL_MODE_STR				= "Режим беспроводной связи"
PREAMBLE_MODE_STR			= "Тип преамбулы"
FRAGTHRESH_STR				= "Порог фрагментации"
RTSTHRESH_STR				= "Порог RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Отключено"
ENABLE_STR 				= "Включено"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Прямое подключение"
INFRASTRUCTURE_STR 			= "Инфраструктура"
AUTO_SELECT_STR 			= "Автовыбор"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Авто"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Испания"
FRANCE_STR 				= "Франция"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Израиль"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Лимит повтора роуминга (с)"
LEISURE_POWER_SAVE_STR			= "Энергосбережение при простое"
AH_BCNINTV_STR 				= "Интервал маяка"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0005] ; Czech
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."


SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanál"
NETWORK_TYPE_STR 			= "Typ sítě"
LED_CONTROL_STR				= "Indikátor LED" 
POWER_SAVE_STR				= "Režim úspory napájení"
WIFI_IBSS_STR				= "Výchozí režim IBSS 11b"
RATE_ADAPTIVE_STR			= "Přizpůsobivé na rychlost"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Měření rádia CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Max. měření offline CCX (0: neomezeno)"
FORCE_PRIORITY_STR			= "Vynucená priorita"
HW_PARA_STR				= "Inic z HwParaFile"
THREE_WIRE_MODE_STR			= "Režim programování Three Wire"
BOARD_TYPE_STR				= "Typ desky"
PROTECTION_MODE_STR			= "Režim ochrany"
TPC_STR					= "Řízení napájení přenosu"
TPC_POLARITY_STR			= "Výběr polarity TPC"
HIGH_POWER_STR				= "Mechanizmus s vysokým výkonem"
INIT_GAIN_STR				= "Počáteční stav zesílení"
CW_MAX_MIN_STR				= "Okno připojení"
PSP_XLINK_STR				= "Režim PSP XLink"
CHANNEL_PLAN_STR			= "Kanálový plán"
WL_MODE_STR				= "Bezdrátový režim"
PREAMBLE_MODE_STR			= "Režim preambule"
FRAGTHRESH_STR				= "Fragmentování prahové hodnoty"
RTSTHRESH_STR				= "Práh RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Deaktivovat"
ENABLE_STR 				= "Aktivovat"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Rychlý_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktura"
AUTO_SELECT_STR 			= "Automatický výběr"
DOMAIN_FROM_EEPROM_STR 			= "DOMÉNA_Z_EEPROM"
AUTO_STR 				= "Auto"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Španělsko"
FRANCE_STR 				= "Francie"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Limit opakovaného pokusu o roaming(s.)"
LEISURE_POWER_SAVE_STR			= "Úsporný režim pro volný čas"
AH_BCNINTV_STR 				= "Interval blikání"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0015] ; Polsih
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR				= "SSID"
CHANNEL_STR				= "Kanał"
NETWORK_TYPE_STR			= "Rozdaj sieci"
LED_CONTROL_STR				= "Wskaźnik LED " 
POWER_SAVE_STR				= "Tryb oszczędzania energii"
WIFI_IBSS_STR				= "Tryb domyślny IBSS 11b "
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"

CCX_RM_STR				= "Pomiar sygnału radiowego CCX "
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Pomiar maks. CCX off-line (0: nieograniczony)"
FORCE_PRIORITY_STR			= "Wymuszone pierwszeństwo"
HW_PARA_STR				= "Inic z HwParaFile"
THREE_WIRE_MODE_STR			= "Trzyprzewodowy tryb programowania"
BOARD_TYPE_STR				= "Rodzaj płyty"
PROTECTION_MODE_STR			= "Tryb zabezpieczenia"
TPC_STR					= "Kontrola mocy nadawanej"
TPC_POLARITY_STR			= "Wybór biegunowości TPC "
HIGH_POWER_STR				= "Mechanizm wysokiej mocy"
INIT_GAIN_STR				= "Stan początkowego wzrostu"
CW_MAX_MIN_STR				= "Okno rywalizacji"
PSP_XLINK_STR				= "Tryb PSP XLink "
CHANNEL_PLAN_STR			= "Plan kanałów"
WL_MODE_STR				= "Tryb bezprzewodowy"
PREAMBLE_MODE_STR			= "Tryb preambuły"
FRAGTHRESH_STR				= "Próg fragmentacji"
RTSTHRESH_STR				= "Próg RTS "
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Wyłącz"
ENABLE_STR 				= "Włącz"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktura"
AUTO_SELECT_STR 			= "Automatyczne wybieranie"
DOMAIN_FROM_EEPROM_STR 			= "DOMENA_Z_EEPROM"
AUTO_STR 				= "Automatyczny"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Hiszpania"
FRANCE_STR 				= "Francja"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Ograniczenie czasu wędrówki (sek.)"
LEISURE_POWER_SAVE_STR			= "Ograniczenie zużycia energii poza pracą"
AH_BCNINTV_STR 				= "Częstotliwość wysyłania ramek"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.001f] ; Turkish
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanal"
NETWORK_TYPE_STR 			= "Ağ Tipi"
LED_CONTROL_STR				= "LED Kontrolü" 
POWER_SAVE_STR				= "Güç Tasarruf Modu"
WIFI_IBSS_STR				= "IBSS Varsayılan 11b Modu"
RATE_ADAPTIVE_STR			= "Uyarlanır Oran"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX Radyo Ölçümü"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Maks Kapalı Hat Ölçümü (0: limitsiz)"
FORCE_PRIORITY_STR			= "Zorunlu Öncelik"
HW_PARA_STR				= "HwParaFile'dan Başlat"
THREE_WIRE_MODE_STR			= "Üç Kablo Programlama Modu"
BOARD_TYPE_STR				= "Kart Tipi"
PROTECTION_MODE_STR			= "Koruma Modu"
TPC_STR					= "İletim Gücü Denetimi"
TPC_POLARITY_STR			= "TPC Kutupsallık Seçimi"
HIGH_POWER_STR				= "Yüksek Güçlü Mekanizma"
INIT_GAIN_STR				= "İlk Edinim Durumu"
CW_MAX_MIN_STR				= "Tartışma Penceresi"
PSP_XLINK_STR				= "PSP XLink Modu"
CHANNEL_PLAN_STR			= "Kanal Planı"
WL_MODE_STR				= "Kablosuz Modu"
PREAMBLE_MODE_STR			= "Başlangıç Modu"
FRAGTHRESH_STR				= "Fragmentasyon Eşiği"
RTSTHRESH_STR				= "RTS Eşiği"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Devredışı Bırak"
ENABLE_STR 				= "Etkinleştir"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"

FAST_PSP_STR 				= "Hızlı_PSP"
AD_HOC_STR 				= "Geçici"
INFRASTRUCTURE_STR 			= "Altyapı"
AUTO_SELECT_STR 			= "Otomatik Seç"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Otomatik"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "İspanya"
FRANCE_STR 				= "Fransa"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "İsrail"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Dolaşım Modu Yeniden Deneme Sınırı (sn)"
LEISURE_POWER_SAVE_STR			= "Boş Zaman Güç Tasarrufu"
AH_BCNINTV_STR 				= "İşaret Aralığı"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.000e] ; Hungarian
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Csatorna"
NETWORK_TYPE_STR 			= "Hálózat típusa"
LED_CONTROL_STR				= "LED-vezérlés" 
POWER_SAVE_STR				= "Energiatakarékos mód"
WIFI_IBSS_STR				= "IBSS alapértelmezett 11b mód"
RATE_ADAPTIVE_STR			= "Adaptív sebességválasztás"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "CCX rádiómérés"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line mérés (0: korlátlan)"
FORCE_PRIORITY_STR			= "Erőltetett elsőbbség"
HW_PARA_STR				= "Inicializálás innen: HwParaFile"
THREE_WIRE_MODE_STR			= "Háromvezetékes programozási mód"
BOARD_TYPE_STR				= "Paneltípus"
PROTECTION_MODE_STR			= "Védett mód"
TPC_STR					= "Sugárzási teljesítményvezérlés"

TPC_POLARITY_STR			= "TPC polaritás választás"
HIGH_POWER_STR				= "Nagyteljesítményű mechanizmus"
INIT_GAIN_STR				= "Kezdeti erősítési állapot"
CW_MAX_MIN_STR				= "Vetélkedési ablak"
PSP_XLINK_STR				= "PSP XLink mód"
CHANNEL_PLAN_STR			= "Csatornaterv"

WL_MODE_STR				= "Vezeték nélküli mód"
PREAMBLE_MODE_STR			= "Előtag mód"
FRAGTHRESH_STR				= "Tördelési küszöb"
RTSTHRESH_STR				= "RTS küszöb"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Letiltás"
ENABLE_STR 				= "Engedélyezés"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infrastruktúra"
AUTO_SELECT_STR 			= "Automata választás"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Automata"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Spanyolország"
FRANCE_STR 				= "Franciaország"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Barangolás újraindításának időkorlátja (mp)"
LEISURE_POWER_SAVE_STR			= "Energiatakarékos mód szórakoztató eszközökhöz"
AH_BCNINTV_STR 				= "Jelzés időköze"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0008] ; Greek
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR 				= "SSID"
CHANNEL_STR				= "Κανάλι"
NETWORK_TYPE_STR 			= "Τύπος Δικτύου"
LED_CONTROL_STR				= "Ενδείξεις λυχνιών LED" 
POWER_SAVE_STR				= "Λειτουργία εξοικονόμησης ενέργειας"
WIFI_IBSS_STR				= "IBSS Προεπιλεγμένη λειτουργία 11b"
RATE_ADAPTIVE_STR			= "Προσαρμόσιμη ταχύτητα"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Ραδιομέτρηση CCX"

CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Μέγιστη μέτρηση εκτός σύνδεσης CCX (0: απεριόριστο)"
FORCE_PRIORITY_STR			= "Εξαναγκασμένη προτεραιότητα"
HW_PARA_STR				= "Αρχικοποίηση από HwParaFile"
THREE_WIRE_MODE_STR			= "Λειτουργία προγραμματισμού τριών καλωδίων"
BOARD_TYPE_STR				= "Τύπος κάρτας"
PROTECTION_MODE_STR			= "Λειτουργία προστασίας"
TPC_STR					= "Έλεγχος μετάδοσης ισχύος"
TPC_POLARITY_STR			= "Επιλογή πολικότητας TPC"
HIGH_POWER_STR				= "Μηχανισμός υψηλής ισχύος"
INIT_GAIN_STR				= "Κατάσταση αρχικού οφέλους"
CW_MAX_MIN_STR				= "Παράθυρο διεκδίκησης"
PSP_XLINK_STR				= "Λειτουργία PSP XLink"
CHANNEL_PLAN_STR			= "Σχέδιο καναλιού"
WL_MODE_STR				= "Λειτουργία ασύρματου"
PREAMBLE_MODE_STR			= "Λειτουργία μπλοκ εισαγωγής"
FRAGTHRESH_STR				= "Κατώφλι τμήματος"
RTSTHRESH_STR				= "Κατώφλι RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Απενεργοποίηση"
ENABLE_STR 				= "Ενεργοποίηση"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Λειτουργία Ad-hoc"
INFRASTRUCTURE_STR 			= "Υποδομή"
AUTO_SELECT_STR 			= "Αυτόματη επιλογή"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Αυτόματο"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Ισπανία"
FRANCE_STR 				= "Γαλλία"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Ισραήλ"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Όριο επαναλήψεων προσπάθειας περιαγωγής (δευτ.)"
LEISURE_POWER_SAVE_STR			= "Εξοικονόμηση ενέργειας σε κατάσταση αδράνειας"
AH_BCNINTV_STR 				= "Διάστημα προειδοποιητικού σήματος"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.001b] ; Slovak
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."


SSID_STR 				= "SSID"
CHANNEL_STR				= "Kanál"
NETWORK_TYPE_STR 			= "Typ siete"
LED_CONTROL_STR				= "LED indikátor" 
POWER_SAVE_STR				= "Režim úspory energie"
WIFI_IBSS_STR				= "Predvolený 11b režim IBSS"
RATE_ADAPTIVE_STR			= "Prispôsobiteľný rýchlosti"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Rádiové meranie pre CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Off line meranie pre CCX Max (0: bez obmedzenia)"
FORCE_PRIORITY_STR			= "Vynútená priorita"
HW_PARA_STR				= "Inicializácia zo súboru HwParaFile"
THREE_WIRE_MODE_STR			= "Trojvodičový režim programovania"
BOARD_TYPE_STR				= "Typ dosky"
PROTECTION_MODE_STR			= "Režim ochrany"
TPC_STR					= "Ovládanie vysielacieho výkonu"
TPC_POLARITY_STR			= "Voľba TPC polarity"
HIGH_POWER_STR				= "Vysoko výkonný mechanizmus"
INIT_GAIN_STR				= "Počiatočný stav získavania"
CW_MAX_MIN_STR				= "Okno pripojenia"
PSP_XLINK_STR				= "Režim linky PSP XLink"
CHANNEL_PLAN_STR			= "Prehľad kanálov"
WL_MODE_STR				= "Bezdrôtový režim"
PREAMBLE_MODE_STR			= "Úvodný režim"
FRAGTHRESH_STR				= "Prahová hodnota pre fragmentáciu"
RTSTHRESH_STR				= "Prahová hodnota pre RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Deaktivovať"
ENABLE_STR 				= "Aktivovať"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Rýchly_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infraštruktúra"
AUTO_SELECT_STR 			= "Automatická voľba"
DOMAIN_FROM_EEPROM_STR 			= "DOMÉNA_Z_EEPROM"
AUTO_STR 				= "Automaticky"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Španielsko"
FRANCE_STR 				= "Francúzsko"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Izrael"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= " Limit(sek) opakovania roamingu "
LEISURE_POWER_SAVE_STR			= " Oddychový úsporný režim "
AH_BCNINTV_STR 				= " Interval majáka "


SSID_STR				= "SSID"
CHANNEL_STR				= "แชนเนล"
NETWORK_TYPE_STR			= "ชนิดเน็ตเวิร์ก"
LED_CONTROL_STR				= "LED ควบคุม" 
POWER_SAVE_STR				= "โหมดประหยัดพลังงาน"
WIFI_IBSS_STR				= "โหมด IBSS เริ่มต้น 11b "
RATE_ADAPTIVE_STR			= "อัตราอะแดปทีฟ"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "การวัดวิทยุ CCX "
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "การวัด CCX ออฟไลน์สูงสุด (0: ไม่จำกัด)"
FORCE_PRIORITY_STR			= "ลำดับความสำคัญที่ถูกบังคับ"
HW_PARA_STR				= "ตั้งค่าเริ่มต้นจาก HwParaFile"
THREE_WIRE_MODE_STR			= "โหมดการโปรแกรม 3 สาย"
BOARD_TYPE_STR				= "ชนิดบอร์ด"
PROTECTION_MODE_STR			= "โหมดการป้องกัน"
TPC_STR					= "ควบคุมพลังงานการส่ง"
TPC_POLARITY_STR			= "เลือกขั้ว TPC "
HIGH_POWER_STR				= "กลไกพลังงานสูง"
INIT_GAIN_STR				= "สถานะเกนเริ่มแรก"
CW_MAX_MIN_STR				= "หน้าต่างการยืนยัน"
PSP_XLINK_STR				= "โหมด PSP XLink "
CHANNEL_PLAN_STR			= "แผนแชนเนล"
WL_MODE_STR				= "โหมดไร้สาย"
PREAMBLE_MODE_STR			= "โหมดส่วนเริ่มต้น"
FRAGTHRESH_STR				= "ขอบเขตชิ้นส่วน"
RTSTHRESH_STR				= "ขอบเขต RTS "
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "ปิดทำงาน"
ENABLE_STR 				= "เปิดทำงาน"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "โครงสร้างพื้นฐาน"
AUTO_SELECT_STR 			= "เลือกอัตโนมัติ"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "อัตโนมัติ"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "สเปน"
FRANCE_STR 				= "ฝรั่งเศส"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "อิสราเอล"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "ขีดจำกัดการลองโรมใหม่ (วินาที)"
LEISURE_POWER_SAVE_STR			= "การประหยัดพลังงานขณะที่ว่าง"
AH_BCNINTV_STR 				= "ช่วงไฟสัญญาณ"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0001] ; Arabic (Saudi Arabia)
Realtek 				= "شركة Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR				= "معرف SSID"
CHANNEL_STR				= "القناة"
NETWORK_TYPE_STR			= "نوع الشبكة"
LED_CONTROL_STR				= "التحكم في مؤشر بيان الحالة" 
POWER_SAVE_STR				= "وضع توفير الطاقة"
WIFI_IBSS_STR				= "وضع 11b الافتراضي لـ IBSS"
RATE_ADAPTIVE_STR			= "مهايئ المعدل"
QOS_STR					= "جودة الخدمة"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "القياس اللاسلكي لـ CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "الحد الأقصى لقياس CCX عند عدم الاتصال (0: غير محدود)"
FORCE_PRIORITY_STR			= "الأولوية الإجبارية"
HW_PARA_STR				= "بدء التهيئة من ملف HwparaFile"
THREE_WIRE_MODE_STR			= "وضع البرمجة ثلاثي الأسلاك"
BOARD_TYPE_STR				= "نوع اللوحة"
PROTECTION_MODE_STR			= "وضع الحماية"
TPC_STR					= "نقل التحكم في الطاقة"
TPC_POLARITY_STR			= "تحديد قطبية TPC"
HIGH_POWER_STR				= "آلية الطاقة المرتفعة"
INIT_GAIN_STR				= "حالة الكسب الأولية"
CW_MAX_MIN_STR				= "نافذة التعارض"
PSP_XLINK_STR				= "وضع PSP XLink"
CHANNEL_PLAN_STR			= "خطة القناة"
WL_MODE_STR				= "الوضع اللاسلكي"
PREAMBLE_MODE_STR			= "وضع الإشارة الابتدائية"
FRAGTHRESH_STR				= "حد التجزئة"
RTSTHRESH_STR				= "حد RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "تعطيل"
ENABLE_STR 				= "تمكين"
CAM_STR 				= "الكامة"
MAX_PSP_STR 				= "الحد الأقصى لـ PSP"
FAST_PSP_STR 				= "PSP سريع"
AD_HOC_STR 				= "عشوائي"
INFRASTRUCTURE_STR 			= "البنية الأساسية"
AUTO_SELECT_STR 			= "تحديد تلقائي"
DOMAIN_FROM_EEPROM_STR 			= "المجال من EEPROM"
AUTO_STR 				= "تلقائي"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "اللجنة الفيدرالية للاتصالات"
IC_STR 					= "دائرة متكاملة"
ETSI_STR 				= "معهد معايير الاتصالات السلكية واللاسلكية"
SPAIN_STR 				= "إسبانيا"
FRANCE_STR 				= "فرنسا"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "إسرائيل"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "حد تكرار التجوال (بالثواني)"
LEISURE_POWER_SAVE_STR			= "توفير الطاقة عند عدم الاستخدام"
AH_BCNINTV_STR 				= "فاصل Beacon الزمني"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.000d] ; Hebrew
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."

SSID_STR				= "SSID"
CHANNEL_STR				= "ערוץ"
NETWORK_TYPE_STR			= "סוג רשת"
LED_CONTROL_STR				= "בקרת נוריות" 
POWER_SAVE_STR				= "מצב חיסכון בצריכת חשמל"
WIFI_IBSS_STR				= "מצב ברירת מחדל 11b ל-IBSS"
RATE_ADAPTIVE_STR			= "קצב מותאם"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "ערך שידור CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "ערך CCX מרבי במצב לא מקוון (0:  ללא הגבלה)"
FORCE_PRIORITY_STR			= "עדיפות מאולצת"
HW_PARA_STR				= "אתחל מקובץ HwParaFile"
THREE_WIRE_MODE_STR			= "מצב תכנות Three Wire"
BOARD_TYPE_STR				= "סוג לוח"
PROTECTION_MODE_STR			= "מצב הגנה"
TPC_STR					= "בקרת הספק שידור"
TPC_POLARITY_STR			= "בחירת קוטביות TPC"
HIGH_POWER_STR				= "מנגנון הספק גבוה"
INIT_GAIN_STR				= "מצב הגבר התחלתי"
CW_MAX_MIN_STR				= "חלון Contention"
PSP_XLINK_STR				= "מצב PSP XLink"
CHANNEL_PLAN_STR			= "תכנון ערוצים"
WL_MODE_STR				= "מצב אלחוטי"
PREAMBLE_MODE_STR			= "מצב מקדים"
FRAGTHRESH_STR				= "סף פיצול"
RTSTHRESH_STR				= "סף RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "חסום"
ENABLE_STR 				= "אפשר"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "MAX_PSP"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "אד הוק"
INFRASTRUCTURE_STR 			= "תשתית"
AUTO_SELECT_STR 			= "בחירה אוטומטית"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "אוטומטי"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "IC"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "ספרד"
FRANCE_STR 				= "צרפת"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "ישראל"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "הגבלת ניסיון חוזר לנדידה (שניות)"
LEISURE_POWER_SAVE_STR			= "מצב חיסכון בחשמל בזמן המתנה"
AH_BCNINTV_STR 				= "מרווח זמן למשואה"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"

;;====================================================================================================================
[Strings.0416] ; Portuguese (Brazil)
Realtek 				= "Realtek Semiconductor Corp."
Lenovo					= "Lenovo Corp."


SSID_STR				= "SSID"
CHANNEL_STR				= "Canal"
NETWORK_TYPE_STR			= "Tipo de Rede"
LED_CONTROL_STR				= "Controle de LED" 
POWER_SAVE_STR				= "Modo de Economia de Energia"
WIFI_IBSS_STR				= "Modo IBSS Default 11b"
RATE_ADAPTIVE_STR			= "Adaptativo à Taxa"
QOS_STR					= "QoS"
WMM_APSD				= "WMM APSD"
CCX_RM_STR				= "Medida de Rádio CCX"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "Medida offline máx. CCX (0: ilimitada)"
FORCE_PRIORITY_STR			= "Prioridade Forçada"
HW_PARA_STR				= "Inicialização de HwParaFile"
THREE_WIRE_MODE_STR			= "Modo de programação de três fios"
BOARD_TYPE_STR				= "Tipo de placa"
PROTECTION_MODE_STR			= "Modo de Proteção"
TPC_STR					= "Controle de Potência de Transmissão"
TPC_POLARITY_STR			= "Seleção de Polaridade TPC"
HIGH_POWER_STR				= "Mecanismo de Alta Potência"
INIT_GAIN_STR				= "Estado de Ganho Inicial"
CW_MAX_MIN_STR				= "Janela de Contenção"
PSP_XLINK_STR				= "Modo PSP XLink"
CHANNEL_PLAN_STR			= "Plano de Canal"

WL_MODE_STR				= "Modo Wireless"
PREAMBLE_MODE_STR			= "Modo de Preâmbulo"
FRAGTHRESH_STR				= "Limite de Fragmentação"
RTSTHRESH_STR				= "Limite RTS"
DOT11_ENABLE_STR			= "802.11d"
11NADHOC_ENABLE_STR			="11n AdHoc"

DISABLE_STR 				= "Desabilitar"
ENABLE_STR 				= "Habilitar"
CAM_STR 				= "CAM"
MAX_PSP_STR 				= "PSP MÁX"
FAST_PSP_STR 				= "Fast_PSP"
AD_HOC_STR 				= "Ad Hoc"
INFRASTRUCTURE_STR 			= "Infra-estrutura"
AUTO_SELECT_STR 			= "Seleção automática"
DOMAIN_FROM_EEPROM_STR 			= "DOMAIN_FROM_EEPROM"
AUTO_STR 				= "Automático"
LONG_PREAMBLE_STR 			= "Long only"
LONG_SHORT_PREAMBLE_STR			= "Short & long"
SHORT_PREAMBLE_STR 			= "Short Preamble"

FCC_STR 				= "FCC"
IC_STR 					= "CI"
ETSI_STR 				= "ETSI"
SPAIN_STR 				= "Espanha"
FRANCE_STR 				= "França"
MKK_STR 				= "MKK"
MKK1_STR 				= "MKK1"
ISRAEL_STR 				= "Israel"
TELEC_STR 				= "TELEC"

IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
Roam_Retry_Limit_STR			= "Limite de Tentativas de Roam (seg)"
LEISURE_POWER_SAVE_STR			= "Economia de Energia de Descanso"
AH_BCNINTV_STR 				= "Intervalo de Sinal"

ROAMING_SENSITIVITY_STR		= "Roaming Sensitivity Level"
HIGH_STR			= "High"
MIDDLE_STR			= "Middle"
LOW_STR				= "Low"

TX_POWER_LEVEL_STR		= "TX Power Level"
HIGH_TX_POWER_STR		= "100 %"			
MIDDLE_TX_POWER_STR		= "75 %"			
LOW_TX_POWER_STR		= "50 %"			
VERY_LOW_TX_POWER_STR		= "20 %"

;;Source disk name
DISKNAME = " Realtek Wireless LAN PCI-E Driver Disk "
RTL8191seva.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc		="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.PEGATRON	="Realtek RTL8191SE 802.11b/g/n Wireless LAN HMC Network"
RTL8191sevb.DeviceDesc.QMI	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"	
RTL8191sevb.DeviceDesc.QMI_EM308	="Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.GBT	="Gigabyte GN-WS21N 802.11n mini WLAN Card"
RTL8192ge.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.DeviceDesc		="Realtek RTL8192SE Wireless LAN 802.11n PCI-E NIC"
RTL8192se.Service.DispName	="Realtek Wireless LAN 802.11n PCI-E NIC NT Driver"
RTL8191seva.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.ASUS_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.ASUS_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191sevb.DeviceDesc.MSI_N	= "Realtek RTL8191SE Wireless LAN 802.11n PCI-E NIC"
RTL8191seva.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191sevb.DeviceDesc.MSI_G	= "Realtek RTL8191SE Wireless LAN Card"
RTL8191seva.DeviceDesc.HP	= "Realtek RTL8191SE 802.11b/g/n WiFi Adapter"	

;; for lenovo
Lenovo.DeviceDesc		="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
Lenovo.DeviceDesc.DispName	="11b/g/n  Wireless LAN Mini-PCI Express Adapter II"
