v2.0.8.3 support both Cx driver and ndis driver

support cards£º
10G£º
pcie£ºRTL8127, RTL8127AP, RTL8127AK, RTL8127AT,  RTL8127ATF
usb£ºRTL8159

5G£º
pcie: RTL8126
usb: RTL8157

2.5G:
pcie: RTL8125£¬RTL8125B, RTL8125D, RTL8125BP, RTL8125K, RTL8125CP
usb:  RTL8156

GIGA
pcie: RTL8168G, RTL8411B, RTL8168H, RTL8168EP, RTL8168FP, add-on cards
usb:  RTL8153

100M:
RTL8106EUS, RTL8107E


For Cable page:
If link is normal, cable length is read from normal register . The error is plus or minus 20 meters in this case.
Or Cable length is read from cable doctor related register . The error is plus or minus 3 meters in this case.