Update Instruction:

1. Unzip the Diags files to the c:\diag folder
2. Copy the firmware file “XXXX.clx” to the c:\diag
3. Run diag -k -f XXXX.clx to program the firmware
4. Once programmed, shutdown the computer and unplug the AC power for 20 seconds.
5. Power on the system
6. run diag -p to show the firmware version information.
