AtlFlashUpdate Tool ReadMe

Overview
==================================================
  This document describes how to use the AtlFlashUpdate Tool to update firmware on AQC1xx-based devices.

System Requirements for firmware update
==================================================
  Windows 10
  AQC1xx-based network card installed:
    AQC-100
    AQC-107
    AQC-108
    AQC-111
  Latest Windows NIC Drivers installed

Usage
=================================================
Interactive mode:
  1) Unzip archive with tool to your hard drive
  2) Open Command line(CMD) and change working directory to extracted folder
  3) Execute "atlflashupdate" at this command line window
  4) Enter number of chosen card and press Enter

Silent mode:
  1) Unzip archive with tool to your hard drive
  2) Open Command line(CMD) and change working directory to extracted folder
  3) Execute "atlflashupdate -s" at this command line window

Help message:
  1) Unzip archive with tool to your hard drive
  2) Open Command line(CMD) and change working directory to extracted folder
  3) Execute "atlflashupdate -h" at this command line window

Support information
==================================================
  For support questions, please contact aqn_support@aquantia.com
  Logs folder is created during update process. This folder contain NIC FW dump prior update and log file. These files are required for tool diagnostic in case of any issues. Please attach them to support request.