============================================================================
                     Fresco Logic F-One Controller Driver
                           Version 1.3.36231.1
                     FUJITSU CLIENT COMPUTING LIMITED
============================================================================
 SOFTWARE INSTRUCTIONS
============================================================================

 This document describes the requirements and reference information
 for the installation of the Fresco Logic F-One Controller Driver.

============================================================================
 Contents of this file
============================================================================

 1. Terms of use
 2. System requirements
 3. Notes
 4. Installing Fresco Logic F-One Controller Driver
 5. Installation confirmation procedure
 6. Uninstalling Fresco Logic F-One Controller Driver
 7. Revision History (Fixed Item)
 8. Copyrights

============================================================================
 1. Terms of use
============================================================================

 Please observe the following terms of use when using this software.
 Please do not use this software if you can not comply with the usage
 conditions.

 1. This software can be used only with the purchased Fujitsu
    computer and the following operating environment.

 2. This software can not be redistributed.
 
 3. It is not possible to remodel this software, reverse engineer,
    disassemble, etc.
    
 4. You can not change any copyright notice concerning this software.
 
 5. As a result of using this software, even if damage occurs,
    our company, and Intel Corporation are not responsible.

============================================================================
 2. System requirements
============================================================================
 
 The following systems are supported by the Fresco Logic F-One Controller
 Driver.

 Operating Systems:
   - Windows 10 64bit
     *For all editions

 Hardware:
   - Wireless cradle

 *You can use this software only with your purchased computer.

============================================================================
 3. Notes
============================================================================

 1. Before using this software, be sure to read the manual attached
    to the main unit.
   
 2. This software is designed and manufactured assuming general applications
    such as general office use, personal use, domestic use, ordinary
    industrial use etc., and it is designed to control nuclear reaction at
    nuclear facilities, automatic flight control of aircraft, aviation
    Extremely high safety, such as traffic control, operation control in
    mass transit system, medical equipment for life support, missile launch
    control in weapons system, etc. are required, and if safety is not
    ensured, directly to life and body. It is not designed and manufactured
    to be used for applications with serious dangers (hereinafter referred
    to as "high safety applications"). Customers should not use this 
    software without taking measures to ensure the safety required for the
    high safety use.
   
 3. Please do not uninstall with "User switching" function with
    multiple users signed in. Please uninstall with only the user
    who is uninstalling signed in.

 4. Not to uninstall older version of driver for updating driver.

============================================================================
 4. Installing Fresco Logic F-One Controller Driver
============================================================================

 1. To install the Fresco Logic F-One Controller Driver, you must sign in
    as an Administrator.

 2. Start "Explorer". 
    Check a box on "Filename extensions" in "View" tab.

 3. Navigate to folder of this software.

 4. Click "FL6KDev-1.3.36231.1.exe" to start this software.

 5. Follow dialogs of installer.

 Installation is now completed.

============================================================================
 5. Installation confirmation procedure
============================================================================

 1. Right click the "Start" button.

 2. Click "Device Manager".

 3. Double click "Universal Serial Bus Devices".

 4. Double click "Fresco Logic F-One Controller"

 5. Click "Driver" tab on "Fresco Logic F-One Controller Properties".

 6. Check "Driver Version" is "1.3.36231.1".

 The software is installed correctly.

============================================================================
 6. Uninstalling Fresco Logic F-One Controller Driver
============================================================================

 1. To uninstall the Fresco Logic F-One Controller Driver, you must
    sign in as an Administrator.

 2. Right click the "Start" button.

 3. Click "Apps and Features".

 4. Click "FL6000 4-Port USB 3.0 F-One Controller".

 5. Click "Uninstall"

 6. Click "Uninstall" on "This app and its related info will be
    uninstalled".

 7. Click "Yes" on "User Account Control".

 8. Restart the computer.

 Uninstallation is now completed.

============================================================================
 7. Revision History (Fixed Item)
============================================================================

 EVersion 1.3.36231.1
   - Fixed BSOD 0x7E.

 EVersion 1.3.35951.1v2
   - Added inf file package

 EVersion 1.3.35951.1
   - New release.
    
============================================================================
 8. Copyrights
============================================================================

 Fresco Logic F-One Controller Driver is developed by Fresco Logic Inc.
 Other company names and product names mentioned are trademarks or
 registered trademarks of each company.
 All other trademarks are the property of their respective owners.

 Copyright FUJITSU CLIENT COMPUTING LIMITED 2019-2020
