Updated firmware to ver. 250708 for ASM4242 and V0206 (GX) for IT8857 to improve compatibility with connected devices.
1. Before using the ASMx4242 FW update tool, Please install Microsoft VC_redist.x64.
2. Please install PD_UPDATE_TOOL_V0206.exe and ASMx4242_FWUpdateV40013_u424250708200011AcmAPDV1.exe from the folder.