MP TOOL Burn Process

1：Click JMMassProd2\_v1\_16\_14\_49.exe TOOL。



2：Click RD Version enter password jmicron。



3：Connect the product which need to burn，wait for PC to connect with the device



4：After connect with the PC , MP TOOL will display the product’s information



5：Choose burn version as below red arrow。



6：Choose FW burn file。（choose the IC [**corresponding**](javascript:;) FW）



7：Click START, then start to burn FW。



8：After burn OK , it will show PASS.

