AtlFlashUpdate Tool
Version 1.2.1
March 31, 2019
Firmware 3.1.81

Description
=======================================================================
AtlFlashUpdate is a tool for updating firmware on AQC100, AQC108, AQC107, AQN100, AQN108, and AQN107

System Requirements
=======================================================================
Windows 10 64-bit
Windows 10 32-bit
Windows 7 64-bit
Windows 7 32-bit

Package contents
=======================================================================
atlflashupdate.exe - main executable, FW update
aqnicnvm64.sys - maintenance driver for interaction with NIC of x64 platforms
aqnicnvm86.sys - maintenance driver for interaction with NIC of x86 platforms
updatedata.xml - configuration file with update information
*.clx - firmware files, which will be burned to the NIC memory

Overview
=======================================================================
This document describes how to use the AtlFlashUpdate Tool to update firmware on Aquantia Network Adapters.

Usage
=======================================================================
Interactive mode:
  1) Unzip archive with tool to your hard drive
  2) Open Command line(CMD) and change working directory to extracted folder
  3) Execute "atlflashupdate" at this command line window
  4) Enter number of chosen card and press Enter

Silent mode:
  1) Unzip archive with tool to your hard drive
  2) Open Command line(CMD) and change working directory to extracted folder
  3) Execute "atlflashupdate -s" at this command line window

Help message:
  1) Unzip archive with tool to your hard drive
  2) Open Command line(CMD) and change working directory to extracted folder
  3) Execute "atlflashupdate -h" at this command line window

Example updating a NIC with 1.5.44 firmware to 3.1.56
=======================================================================

1. Open DOS Window as Admin
Microsoft Windows [Version 10.0.17763.437]
(c) 2018 Microsoft Corporation. All rights reserved. 

2. Go to folder that has the files extracted

C:\WINDOWS\system32>cd\AtlFlashUpdate

C:\AtlFlashUpdate>dir
Volume in drive C has no label.
Volume Serial Number is 92A2-6452

Directory of C:\AtlFlashUpdate
09/18/2018 03:35 AM 2,097,152 AQC108_3.1.56.clx
04/16/2019 05:02 AM 89,784 aqnicnvm64.sys
04/16/2019 05:02 AM 77,864 aqnicnvm86.sys
03/31/2019 10:42 PM 492,544 atlflashupdate.exe
04/17/2019 03:01 AM 53 content.txt
04/17/2019 08:14 AM 1,526 readme.txt
04/18/2019 03:56 PM 457 updatedata.xml
04/17/2019 03:01 AM 13 version.txt

3. Run the executable program atlflashupdate

C:\AtlFlashUpdate>atlflashupdate.exe

Aquantia AQtion Firmware Update Tool [Version 1.2.1]

________________________________________________________________________________________________________
1 Aquantia AQtion 5Gbit Network Adapter 1.5.44 Available: 3.1.56 D108-00011D6A 00:17:B6:00:13:E9
________________________________________________________________________________________________________
*** Important note ***
The network connection may be dropped during the update process.
Please complete all network activity before updating.

4. Select the adapter that has the older firmware (1.5.44)

Enter adapter number or 'q' for quit without update >
1

===
+ Adapter: Aquantia AQtion 5Gbit Network Adapter
|-- HWID: VEN_1D6A&DEV_D108&SUBSYS_00011D6A
|-- Backing up... [OK]
|-- Updating... [OK]
|-- New firmware version: 3.1.56
|-- Trying to reload firmware... [OK]
|-- Restarting device driver... [OK]
===

Firmware update finished!

Press any key...

C:\AtlFlashUpdate> 5. If you run the program again, you can see the card has the firmware 3.1.56 installed.

C:\AtlFlashUpdate>atlflashupdate.exe

Aquantia AQtion Firmware Update Tool [Version 1.2.1]
________________________________________________________________________________________________________
1 Aquantia AQtion 5Gbit Network Adapter 3.1.56 Not required D108-00011D6A 00:17:B6:00:13:E9
________________________________________________________________________________________________________

No adapters can be updated

Press any key...

Support information
=======================================================================
For support questions, please contact aqn_support@aquantia.com
A folder \logs will be created during the update process.
Zip up the folder and email the file to Aquantia for review.